Linux Install AVC Program

1. Download the Linux SMFL library from either the GitHub or the website: <https://www.sfml-dev.org/download/sfml/2.5.1/>
2. Go to your downloads folder and extract it
3. Change the path in the make file for the robot and server to your usernames download folder
4. Download all the files required from the GitHub
5. Extract them and locate the robot and server.cpp files
6. Open the robot.cpp and server.cpp file in Geany
7. Click build at the top and then make both files
8. Done