To be able to do Project 3 on Windows there was a different process to install the necessary files compared to Linux and Mac.

To do the coding for the project, Geany and MinGW must be installed. MinGW helps Geany when doing the coding. The following files needed to be downloaded to do the project.







As well as that, dll files from the bin folder which is located in the MinGW folder had to be put into the AVC\_robot and AVC\_server folder. With all of that sorted out, there was one more step to make sure the coding was able to be built properly. Within Geany and underneath ‘build’ there is another button called ‘set build commands’. Within that there must be a change in ‘Make’. This must be changed to the following below.



If this is done correctly, then the code will be able to run properly.